LEDs-

Fetch-decode-execute: 1 meter

Register name plates:

Red 1 meter

Blue 2 meters

Registers needed:

MDR

MAR

AX

BX

IR

Changes to leds should tank place over 2 frames

Should come forward to: y -0.1

Mem integration-

Use 2 stacked 4 cluster gantrys